**4G WIFI IP Camera Instruction**

A：Offline and recharge function

Self checking and recovery when being offline : when being offline from the WAN, the device will self-checking every two minutes and reconnect automatically ( if there’s no MB of transferred data in SIM card, camera will reconnect automatically after recharging)

B：Optional connection to Internet

 1. Auto connection mode ( under Auto connection mode, the camera will prefer to select WIFI if WIFI and 4G are available for the camera )

2. 3G/4G Mode: Fixed 3G/4G to Internet

3. WIFI Mode: select available WIFI with password

to Internet

C：How to make camera connected Internet with 4G

or WIFI With 3G/4G SIM card


Press SIM card to SIM card slot without any setting

2. With WIFI ( camera can be set wireless parameter on phone,


table, pr laptop) Take laptop for example, connect laptop to the

WIFI named like MIFI-XX (default password :1234567890)


② Open IE browser, type in 192.168.100.1 to access camera , password is admin




③Choose WIFI Setting




④Choose Internet WIFI




⑤ Click “Add”



⑥Choose the WIFI you want to connect, type in the password if you need , then “ Success” page will show up





D：Manage camera by message ( sending message to the number of SIM installed in camera)

1.Open 4G command：\*#01#

2.Close 4G commaned：\*#02#

3.Open WIFI function：\*#03#

4.Close WIFI function：\*#04#

5.Restarting camera：\*#05#

6.Resetting camera to factory default： \*#06#

7.Switch to Auto Connection Mode：\*#07#,dialpref ------ prefer to 4G

\*#07#,wifipref ------ prefer to WIFI



8.Connect/Disconnect the hotspot from camera ：

\*#08#,MIFI\_0123,1234567890,add ---(connect hotspot named(SSID) MIFI-XX, password: 1234567890)


\*#08#,MIFI\_0123,1234567890,delete-----(disconnect hotspot named(SSID) MIFI-XX, password: 1234567890)


**E： How to add camera on smartphone**

Download camhi ( for IOS and android ) from APP store，open it and click add

2.Click Scan QR code , then scan the QR on the cover to add camera, type in password( admin by default ) . click Done.







If the camera and phone are under the same WIFI, you can click “ Search camera from LAN” to add camera